Router 4 running-configuration

R4#show run

Building configuration...

Current configuration : 1860 bytes

! Last configuration change at 19:53:34 UTC Wed Sep 7 2022

version 15.5

service timestamps debug datetime msec

service timestamps log datetime msec

no platform punt-keepalive disable-kernel-core

hostname R4

boot-start-marker

boot-end-marker

vrf definition Mgmt-intf

address-family ipv4

exit-address-family

address-family ipv6

exit-address-family

no aaa new-model

ipv6 unicast-routing

subscriber templating

vtp domain cisco

vtp mode transparent

multilink bundle-name authenticated

license udi pid ISR4321/K9 sn FDO21442B21

spanning-tree extend system-id

redundancy

mode none

vlan internal allocation policy ascending

vlan 10,20

interface GigabitEthernet0/0/0

ip address 10.0.4.1 255.255.255.0

negotiation auto

ipv6 address FE80::1 link-local

ipv6 address 2001:DB8:ACAD:5::2/64

ipv6 ospf 1 area 0

interface GigabitEthernet0/0/1

ip address 10.0.3.2 255.255.255.0

negotiation auto

ipv6 address FE80::2 link-local

ipv6 address 2001:DB8:ACAD:4::1/64

ipv6 ospf 1 area 0

interface Serial0/1/0

no ip address

shutdown

interface Serial0/1/1

no ip address

shutdown

interface GigabitEthernet0/2/0

no ip address

shutdown

negotiation auto

interface GigabitEthernet0/2/1

no ip address

shutdown

negotiation auto

interface GigabitEthernet0

vrf forwarding Mgmt-intf

no ip address

shutdown

negotiation auto

interface Vlan1

no ip address

shutdown

router ospfv3 1

router-id 4.4.4.4

address-family ipv6 unicast

exit-address-family

router ospf 1

network 10.0.3.0 0.0.0.255 area 0

network 10.0.4.0 0.0.0.255 area 0

ip forward-protocol nd

no ip http server

no ip http secure-server

ip tftp source-interface GigabitEthernet0

control-plane

line con 0

stopbits 1

line aux 0

stopbits 1

line vty 0 4

login

end

Router 4 IPv4 and IPv6 routes:

R4#show ip route

Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP

D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area

N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2

E1 - OSPF external type 1, E2 - OSPF external type 2

i - IS-IS, su - IS-IS summary, L1 - IS-IS level-1, L2 - IS-IS level-2

ia - IS-IS inter area, \* - candidate default, U - per-user static route

o - ODR, P - periodic downloaded static route, H - NHRP, l - LISP

a - application route

+ - replicated route, % - next hop override, p - overrides from PfR

Gateway of last resort is not set

10.0.0.0/8 is variably subnetted, 8 subnets, 2 masks

O 10.0.0.0/24 [110/4] via 10.0.3.1, 00:06:44, GigabitEthernet0/0/1

O 10.0.1.0/24 [110/3] via 10.0.3.1, 00:19:40, GigabitEthernet0/0/1

O 10.0.2.0/24 [110/2] via 10.0.3.1, 00:19:40, GigabitEthernet0/0/1

C 10.0.3.0/24 is directly connected, GigabitEthernet0/0/1

L 10.0.3.2/32 is directly connected, GigabitEthernet0/0/1

C 10.0.4.0/24 is directly connected, GigabitEthernet0/0/0

L 10.0.4.1/32 is directly connected, GigabitEthernet0/0/0

O 10.0.5.0/24 [110/2] via 10.0.4.2, 00:06:44, GigabitEthernet0/0/0

R4#show ipv6 route

IPv6 Routing Table - default - 9 entries

Codes: C - Connected, L - Local, S - Static, U - Per-user Static route

B - BGP, R - RIP, I1 - ISIS L1, I2 - ISIS L2

IA - ISIS interarea, IS - ISIS summary, D - EIGRP, EX - EIGRP external

ND - ND Default, NDp - ND Prefix, DCE - Destination, NDr - Redirect

O - OSPF Intra, OI - OSPF Inter, OE1 - OSPF ext 1, OE2 - OSPF ext 2

ON1 - OSPF NSSA ext 1, ON2 - OSPF NSSA ext 2, a - Application

O 2001:DB8:ACAD:1::/64 [110/3]

via FE80::1, GigabitEthernet0/0/1

O 2001:DB8:ACAD:2::/64 [110/4]

via FE80::1, GigabitEthernet0/0/1

O 2001:DB8:ACAD:3::/64 [110/2]

via FE80::1, GigabitEthernet0/0/1

C 2001:DB8:ACAD:4::/64 [0/0]

via GigabitEthernet0/0/1, directly connected

L 2001:DB8:ACAD:4::1/128 [0/0]

via GigabitEthernet0/0/1, receive

C 2001:DB8:ACAD:5::/64 [0/0]

via GigabitEthernet0/0/0, directly connected

L 2001:DB8:ACAD:5::2/128 [0/0]

via GigabitEthernet0/0/0, receive

O 2001:DB8:ACAD:6::/64 [110/2]

via FE80::2, GigabitEthernet0/0/0

L FF00::/8 [0/0]

via Null0, receive